|  |  |  |
| --- | --- | --- |
| **Compliance** | **YES/NO** | **COMMENTS** |
| **Mandatory Minimum Technical Characteristics of digital portable radios** | | |
| Type: Digital |  |  |
| Frequency band: UHF |  |  |
| Frequency range: 403-470MHz |  |  |
| Minimum number of channels: 16 |  |  |
| 1/4W |  |  |
| Ingress protection marking:   1. IP 54 2. IEC60529 |  |  |
| **Mandatory Minimum Physical Characteristics of portable radios** | | |
| Without front LCD and front keyboard |  |  |
| Operating Manual in Portuguese and English |  |  |
| **Radio Accessories** | | |
| Antenna |  |  |
| Battery: Li-Ion 1400mAh |  |  |
| Average life with Li-Ion 1400mAh: 8hrs |  |  |
| Chargers |  |  |
| 3” Belt clip |  |  |
| Technical assistance |  |  |
| Support/assistance to arrange the licence/frequency with ANACOM |  |  |
| Programing of radios according to the licence issued by ANACOM |  |  |